|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| mb1.jpg | Intel DH77EB Motherboard | * Micro-ATX Form Factor * LGA 1155 Socket Type * Intel H77 Chipset * RAID Controller: Intel H77 Chipset * 4 Memory Slots * Maximum 32 GB DDR3 * Dual Channel DIMM Memory | **Rs. 6930** | 0 | **Rs. 6930** |
| mb2.jpg | Intel DX79TO Motherboard | * ATX Form Factor * LGA2011 Socket Type * Intel X79 Express Chipset * RAID Controller: Intel X79 Express Chipset * 8 memory Slots * Maximum 64 GB DDR3 * Dual Channel DIMM Memory | **Rs. 17280** | 0 | **Rs. 17280** |
| mb3.jpg | Intel DH67CL Motherboard | * ATX Form Factor * LGA 1155 Socket Type * Intel H67 * 4 Memory Slots * Maximum 32 GB DDR3 * Dual Channel DIMM Memory * 1 HDMI Ports | **Rs. 13900** | 20 | **Rs. 10999** |
| mb4.jpg | ASUS P9X79 PRO Motherboard | * ATX Form Factor * LGA 2011 Socket Type * Intel X79 Chipset * Raid Controller: Intel X79 * 8 Memory Slots * Maximum 64 GB DDR3 * Quad Channel DIMM Memory | **Rs. 30300** | 15 | **Rs. 25699** |
| mb5.jpg | Asus Z87-K Motherboard | * Intel Z87 Chipset * Dual Channel DIMM Memory * ATX Form Factor * 4 Memory Slots * 1 HDMI Port * LGA 1150 Socket Type * Maximum 32 GB DDR3 | **Rs. 14925** | 16 | **Rs. 12518** |
| mb6.jpg | ASUS P8B75-M LX Motherboard | * 2 Memory Slots * Intel B75 Chipset * Micro-ATX Form Factor * LGA 1155 Socket Type * Maximum 16 GB DDR3 * Dual Channel DIMM Memory * 5 SATA 3Gb/s Headers with Intel B75 chipset Controller | **Rs. 6000** | 5 | **Rs. 5690** |
| mb7.jpg | Gigabyte G1 Sniper 5 Moherboard | * E-ATX Form Factor * Marvell 88SE9230 * LGA 1150 Socket Type * Intel Z87 Chipset * Maximum 32 GB DDR3 * 4 Memory Slots * RAID Controller: Intel Z87 * Dual Channel DIMM Memory | **Rs. 36180** | 0 | **Rs. 36180** |
| mb8.jpg | Gigabyte H87-D3H Motherboard | * Dual Channel DIMM Memory * ATX Form Factor * Intel H87 Chipset * Maximum 32 GB DDR3 * 1 HDMI Port * LGA 1150 Socket Type * 4 Memory Slots | **Rs. 14999** | 38 | **Rs. 9150** |
| mb9.jpg | Gigabyte GA-B75M-D3H Motherboard | * Micro-ATX Form Factor * LGA 1155 Socket Type * Intel B75 Express Chipset * 4 Memory Slots * Maximum 32 GB DDR3 * Dual Channel DIMM Memory * 1 HDMI Ports | **Rs. 4850** | 0 | **Rs. 4850** |
| mb10.jpg | ASRock Z77 Extreme4 Motherboard | * ATX Form Factor * LGA 1155 Socket Type * Intel Z77 Chipset * RAID Controller: Intel Z77 Chipset * 4 Memory Slots * Maximum 32 GB DDR3 * Dual Channel DIMM Memory | **Rs. 17100** | 29 | **Rs. 12100** |
| mb11.jpg | ASRock H71M-DGS Motherboard | * Micro-ATX Form Factor * LGA 1155 Socket Type * 2 Memory Slots * Maximum 16 GB DDR3 * Intel H61 Chipset * Dual Channel DIMM Memory * 5.1 Audio I/O Channels | **Rs. 4990** | 30 | **Rs. 3475** |
| mb12.jpg | ASRock Z87 OC Formula Motherboard | * ntel Z87 Chipset * 4 Memory Slots * 2 HDMI Port * E-ATX Form Factor * Dual Channel DIMM Memory * LGA 1150 Socket Type * Maximum 32 GB DDR3 | **Rs. 28812** | 0 | **Rs. 28812** |